|  |  |
| --- | --- |
| **CHECKPOINTS** | **SIGN** |
| Install MLG chocks *(N/A if aircraft is on fuselage jacks)* |  |
| Statically ground aircraft |  |
| Place oil/fuel spillage container under aircraft |  |
| Install NLG safety pin (1) |  |
| Install MLG safety pins (2) |  |
| Install pitot cover (1) |  |
| Arresting hook lowered or safety pin installed  |  |
| Install ejection seat safety pins (1) |  |
| Disconnect aircraft battery  | N/A |
| Install engine inlet covers |  |
| Install dragchute safetypins |  |
| Check jacks for correct position for LG operation |  |
| Check gear doors switch position (OPEN) |  |
| Check lock safety ring on jacks for right position |  |
| HUD EU fuse – Pulled |  |
| HUD FAN fuse – Pulled |  |
| All HEATER fuses in cockpit – Pulled |  |
| FUEL BOOST PUMP L/H and R/H, crossfeed switch - Off |  |
| FUEL SHUT-OFF L/H, R/H closed position with guard down |  |
| Check that Flap position corresponds to Flap switch position |  |
| All other cockpit switches in OFF/NORMAL position |  |
| *Before applying Hydraulic power:*  |  |
| Ensure clearance to equipment and obstacles, set out Cone barrier and Red Warning light. |  |

**Date:\_\_\_\_\_\_\_\_\_\_\_ SIGN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Interne referanser**

|  |  |
| --- | --- |
|   |   |

**Eksterne referanser**

|  |
| --- |
|   |