|  |  |  |
| --- | --- | --- |
| **CHECKPOINTS** | **Position** | **SIGN** |
| Helicopter weight on skids |  |  |
| Statically ground aircraft |  |  |
| Place oil/fuel spillage container under aircraft |  |  |
| Insert plugs in fuselage static ports L/H and R/H |  |  |
| Install pitot cover (1) |  |  |
| Disconnect aircraft battery  |  |  |
| Install engine inlet and exhaust covers  |  |  |
| Fuel shut-off handle in cockpit  | Down |  |
| Rotor brake handle in cockpit  | Down |  |
| Radio Master switch in cockpit  | Off |  |
| Pitot heat c/b in cockpit  | Out |  |
| ELT c/b in cockpit  | Out |  |
| All other cockpit switches in OFF/NORMAL position | Off/Norm |  |
| Com 1 + XPDR + TCAD c/b ( cargo comp)  | Out |  |
| RAD ALT c/b ( cargo comp)  | Out |  |
| Land LT cont c/b ( cargo comp)  | Out |  |
| Strobe light c/b ( cargo comp)  | Out |  |
| Hyd cut off c/b ( cargo comp)  | Out |  |
| Hour meter c/b ( cargo comp)  | Out |  |

Dato:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Sign:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Interne referanser**

|  |  |
| --- | --- |
|   |   |

**Eksterne referanser**

|  |
| --- |
|   |